1. Installing on Decks Too Low Sloped

2. No Drip Edge

3. Starter Problems

4. No Leak Barrier at All Spots

5. Nailing Problems

6. Valley Problems

7. Flashing Problems

8. No Chimney Crickets

9. Improper Ventilation

10. Wrong Ridge Caps